(kicad_pcb (version 20171130) (host pcbnew 5.1.2)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 29)
    (nets 51)
  )

  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 /RTS)
  (net 4 +3V3)
  (net 5 +5V)
  (net 6 "Net-(C9-Pad2)")
  (net 7 /DTR)
  (net 8 /TX)
  (net 9 /RX)
  (net 10 "Net-(LS1-Pad1)")
  (net 11 "Net-(LS2-Pad1)")
  (net 12 /LED_DATA)
  (net 13 /LRCK)
  (net 14 /BCLK)
  (net 15 /I2SD)
  (net 16 /SDA)
  (net 17 /SCL)
  (net 18 "Net-(U2-Pad4)")
  (net 19 "Net-(U2-Pad3)")
  (net 20 "Net-(U2-Pad1)")
  (net 21 /MISO)
  (net 22 /SCLK)
  (net 23 /MOSI)
  (net 24 /CS)
  (net 25 "Net-(C9-Pad1)")
  (net 26 "Net-(C10-Pad2)")
  (net 27 "Net-(C11-Pad1)")
  (net 28 "Net-(J3-Pad8)")
  (net 29 "Net-(U3-Pad4)")
  (net 30 "Net-(U3-Pad5)")
  (net 31 "Net-(U3-Pad6)")
  (net 32 "Net-(U3-Pad7)")
  (net 33 "Net-(U3-Pad9)")
  (net 34 "Net-(U3-Pad12)")
  (net 35 "Net-(U3-Pad13)")
  (net 36 "Net-(U3-Pad14)")
  (net 37 "Net-(U3-Pad16)")
  (net 38 "Net-(U3-Pad17)")
  (net 39 "Net-(U3-Pad18)")
  (net 40 "Net-(U3-Pad19)")
  (net 41 "Net-(U3-Pad20)")
  (net 42 "Net-(U3-Pad21)")
  (net 43 "Net-(U3-Pad22)")
  (net 44 "Net-(U3-Pad23)")
  (net 45 "Net-(U3-Pad24)")
  (net 46 "Net-(U3-Pad27)")
  (net 47 "Net-(U3-Pad28)")
  (net 48 "Net-(U3-Pad32)")
  (net 49 "Net-(D1-Pad4)")
  (net 50 "Net-(D2-Pad4)")

  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BCLK)
    (add_net /CS)
    (add_net /DTR)
    (add_net /I2SD)
    (add_net /LED_DATA)
    (add_net /LRCK)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RTS)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SCLK)
    (add_net /SDA)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(LS1-Pad1)")
    (add_net "Net-(LS2-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad24)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad32)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad9)")
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD) (tstamp 5DD1EAD6)
    (at 99.395 68.065)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /5DD5B861)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(D2-Pad4)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 5DD1EA03)
    (at 86.315 74.765)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (path /5DD005F5)
    (fp_text reference J7 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04_Male (at 4.385 9.89) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 9.4) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 10.55 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 8.95) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.95) (end 4.1 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.33) (end 1.44 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 8.89) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 8.89) (end 1.5 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 5DD1E78A)
    (at 86.315 62.515)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (path /5DCFAA17)
    (fp_text reference J6 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04_Male (at 4.385 9.89) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 9.4) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 10.55 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 8.95) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.95) (end 4.1 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.33) (end 1.44 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 8.89) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 8.89) (end 1.5 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 5DD1E511)
    (at 72.915 74.765)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (path /5DCF5127)
    (fp_text reference J5 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04_Male (at 4.385 9.89) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 9.4) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 10.55 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 8.95) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.95) (end 4.1 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.33) (end 1.44 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 8.89) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 8.89) (end 1.5 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 5DD1E298)
    (at 72.915 62.515)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (path /5DCDEB7C)
    (fp_text reference J4 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04_Male (at 4.385 9.89) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 9.4) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 10.55 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 8.95) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.95) (end 4.1 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.33) (end 1.44 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 8.89) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 8.89) (end 1.5 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B263) (tstamp 5DD1DE27)
    (at 110.02 63.5)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (path /5DD1E4E8)
    (attr smd)
    (fp_text reference D2 (at 0 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812 (at 0 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.65 2.75) (end 3.65 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 2.75) (end 3.65 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.5) (end 1.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.45 2.75) (end 3.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (pad 3 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D2-Pad4)"))
    (pad 2 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B263) (tstamp 5DD1DD85)
    (at 101.6 63.5)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (path /5DD1D6E4)
    (attr smd)
    (fp_text reference D1 (at 0 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812 (at 0 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.65 2.75) (end 3.65 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 2.75) (end 3.65 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.5) (end 1.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.45 2.75) (end 3.45 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (pad 3 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /LED_DATA))
    (pad 1 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Card:microSD_HC_Hirose_DM3AT-SF-PEJM5 (layer B.Cu) (tedit 5A1DBFB5) (tstamp 5DC4229D)
    (at 148 79)
    (descr "Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)")
    (tags "Micro SD")
    (path /5DC3F3D7)
    (attr smd)
    (fp_text reference J3 (at -0.075 9.525) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Micro_SD_Card (at -0.075 -9.575) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start -5.425 -13.225) (end -5.425 -13.725) (angle -90) (layer B.Fab) (width 0.1))
    (fp_arc (start 4.575 -13.225) (end 5.075 -13.225) (angle -90) (layer B.Fab) (width 0.1))
    (fp_arc (start -5.425 -9.225) (end -5.425 -9.725) (angle -90) (layer B.Fab) (width 0.1))
    (fp_arc (start 4.575 -9.225) (end 5.075 -9.225) (angle -90) (layer B.Fab) (width 0.1))
    (fp_line (start 3.275 1.525) (end 2.7 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.275 2.025) (end 2 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.275 2.525) (end 1.3 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 2.825 2.725) (end 0.6 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 2.125 2.725) (end -0.1 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 1.425 2.725) (end -0.8 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 0.725 2.725) (end -1.5 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 0.025 2.725) (end -2.2 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start -0.675 2.725) (end -2.9 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start -1.375 2.725) (end -3.6 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start -2.075 2.725) (end -4.3 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start -5.925 -8.325) (end -5.925 -13.225) (layer B.Fab) (width 0.1))
    (fp_line (start 5.075 -13.225) (end 5.075 -8.325) (layer B.Fab) (width 0.1))
    (fp_line (start -5.425 -13.725) (end 4.575 -13.725) (layer B.Fab) (width 0.1))
    (fp_line (start -5.425 -9.725) (end 4.575 -9.725) (layer B.Fab) (width 0.1))
    (fp_line (start 2.51 -7.975) (end -3.915 -7.975) (layer B.Fab) (width 0.1))
    (fp_line (start 6.925 7.825) (end -6.925 7.825) (layer B.Fab) (width 0.1))
    (fp_line (start 6.925 -8.125) (end 6.925 7.825) (layer B.Fab) (width 0.1))
    (fp_line (start -6.925 -8.125) (end -6.925 7.825) (layer B.Fab) (width 0.1))
    (fp_line (start 5.285 -8.325) (end 3.035 -8.325) (layer B.Fab) (width 0.1))
    (fp_line (start 5.285 -8.325) (end 5.485 -8.125) (layer B.Fab) (width 0.1))
    (fp_line (start 3.035 -8.325) (end 2.51 -7.975) (layer B.Fab) (width 0.1))
    (fp_line (start -5.915 -8.325) (end -6.115 -8.125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.915 -8.125) (end -4.115 -8.325) (layer B.Fab) (width 0.1))
    (fp_line (start -4.115 -8.325) (end -5.915 -8.325) (layer B.Fab) (width 0.1))
    (fp_line (start 5.485 -8.125) (end 6.925 -8.125) (layer B.Fab) (width 0.1))
    (fp_line (start -6.115 -8.125) (end -6.925 -8.125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.915 -8.125) (end -3.915 -7.975) (layer B.Fab) (width 0.1))
    (fp_line (start -5.425 2.725) (end 3.275 2.725) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.275 2.725) (end 3.275 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.275 1.125) (end -5.425 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start 2.925 -6.975) (end 5.475 -6.975) (layer Dwgs.User) (width 0.1))
    (fp_line (start 5.475 -6.975) (end 5.475 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 5.475 -8.325) (end 2.925 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 2.925 -8.325) (end 2.925 -6.975) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 1.425) (end -5.425 1.425) (layer Dwgs.User) (width 0.1))
    (fp_line (start -5.425 2.725) (end -5.425 -6.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -5.425 -6.175) (end -6.125 -6.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -6.175) (end -6.125 1.425) (layer Dwgs.User) (width 0.1))
    (fp_line (start -7.225 7.275) (end -6.475 7.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 7.275) (end -6.475 -0.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 -0.775) (end -7.225 -0.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -7.225 -0.775) (end -7.225 7.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -7.82 8.82) (end 7.88 8.82) (layer B.CrtYd) (width 0.05))
    (fp_line (start 7.88 8.82) (end 7.88 -8.88) (layer B.CrtYd) (width 0.05))
    (fp_line (start 7.88 -8.88) (end -7.82 -8.88) (layer B.CrtYd) (width 0.05))
    (fp_line (start -7.82 -8.88) (end -7.82 8.82) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.075 7.885) (end 6.995 7.885) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.995 7.885) (end 6.995 -6.125) (layer B.SilkS) (width 0.12))
    (fp_line (start -6.525 7.885) (end -6.975 7.885) (layer B.SilkS) (width 0.12))
    (fp_line (start -6.975 7.885) (end -6.975 4.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.315 -8.385) (end 3.005 -8.385) (layer B.SilkS) (width 0.12))
    (fp_line (start -5.945 -8.385) (end -4.085 -8.385) (layer B.SilkS) (width 0.12))
    (fp_line (start -5.945 -8.385) (end -6.145 -8.185) (layer B.SilkS) (width 0.12))
    (fp_line (start -6.975 2.575) (end -6.975 -2.125) (layer B.SilkS) (width 0.12))
    (fp_line (start -6.975 -3.425) (end -6.975 -5.225) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.875 -8.035) (end 2.495 -8.035) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.875 -8.035) (end -3.875 -8.185) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.085 -8.385) (end -3.875 -8.185) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.315 -8.385) (end 5.515 -8.185) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.515 -8.185) (end 5.775 -8.185) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.005 -8.385) (end 2.495 -8.035) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.475 -6.975) (end 4.675 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 4.975 -6.975) (end 4.175 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 4.475 -6.975) (end 3.675 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.975 -6.975) (end 3.175 -8.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start 3.475 -6.975) (end 2.925 -7.875) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 7.275) (end -7.225 6.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 6.775) (end -7.225 6.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 6.275) (end -7.225 5.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 5.775) (end -7.225 5.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 5.275) (end -7.225 4.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 4.775) (end -7.225 4.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 4.275) (end -7.225 3.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 3.775) (end -7.225 3.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 3.275) (end -7.225 2.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 2.775) (end -7.225 2.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 2.275) (end -7.225 1.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 1.775) (end -7.225 1.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 1.275) (end -7.225 0.775) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 0.775) (end -7.225 0.275) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 0.275) (end -7.225 -0.225) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.475 -0.225) (end -7.225 -0.725) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -6.175) (end -5.425 -5.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -5.675) (end -5.425 -5.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -5.175) (end -5.425 -4.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -4.675) (end -5.425 -4.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -4.175) (end -5.425 -3.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -3.675) (end -5.425 -3.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -3.175) (end -5.425 -2.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -2.675) (end -5.425 -2.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -2.175) (end -5.425 -1.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -1.675) (end -5.425 -1.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -1.175) (end -5.425 -0.675) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -0.675) (end -5.425 -0.175) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 -0.175) (end -5.425 0.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 0.325) (end -5.425 0.825) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 1.325) (end -5.975 1.425) (layer Dwgs.User) (width 0.1))
    (fp_line (start -6.125 0.825) (end -5.425 1.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start -5.425 1.325) (end -3.475 2.725) (layer Dwgs.User) (width 0.1))
    (fp_line (start -2.775 2.725) (end -5 1.125) (layer Dwgs.User) (width 0.1))
    (fp_line (start -4.875 2.725) (end -5.425 2.325) (layer Dwgs.User) (width 0.1))
    (fp_line (start -4.175 2.725) (end -5.425 1.825) (layer Dwgs.User) (width 0.1))
    (fp_text user KEEPOUT (at -5.775 -2.375 -90) (layer Cmts.User)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_text user KEEPOUT (at -6.85 3.25 -90) (layer Cmts.User)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_text user KEEPOUT (at 4.2 -7.65) (layer Cmts.User)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_text user %R (at -0.075 -0.375) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.1)) (justify mirror))
    )
    (fp_text user KEEPOUT (at -1.075 1.925) (layer Cmts.User)
      (effects (font (size 1 1) (thickness 0.1)))
    )
    (pad 11 smd rect (at 6.675 -7.375) (size 1.3 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -6.825 -6.925) (size 1 2.8) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -6.825 -2.775) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -6.825 3.425) (size 1 1.2) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 4.325 7.725) (size 1 1.2) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.825 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 /MISO))
    (pad 6 smd rect (at -2.725 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.625 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 22 /SCLK))
    (pad 4 smd rect (at -0.525 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 0.575 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.675 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 23 /MOSI))
    (pad 1 smd rect (at 2.775 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 24 /CS))
    (pad 8 smd rect (at -4.925 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J3-Pad8)"))
    (pad 9 smd rect (at -5.875 7.725) (size 0.7 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5A02FF57) (tstamp 5DC425ED)
    (at 59.5 42.65 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (path /5DC41BA9)
    (attr smd)
    (fp_text reference U1 (at 0 4.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value AP7361C-33E (at 0 -4.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.85 3.35) (end 1.85 -3.35) (layer B.Fab) (width 0.1))
    (fp_line (start -1.85 -3.35) (end 1.85 -3.35) (layer B.Fab) (width 0.1))
    (fp_line (start -4.1 3.41) (end 1.91 3.41) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.85 3.35) (end 1.85 3.35) (layer B.Fab) (width 0.1))
    (fp_line (start -1.85 -3.41) (end 1.91 -3.41) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.85 2.35) (end -1.85 -3.35) (layer B.Fab) (width 0.1))
    (fp_line (start -1.85 2.35) (end -0.85 3.35) (layer B.Fab) (width 0.1))
    (fp_line (start -4.4 3.6) (end -4.4 -3.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 -3.6) (end 4.4 -3.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.4 -3.6) (end 4.4 3.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.4 3.6) (end -4.4 3.6) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.91 3.41) (end 1.91 2.15) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.91 -3.41) (end 1.91 -2.15) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
    )
    (pad 1 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 3 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm (layer B.Cu) (tedit 5A02F25C) (tstamp 5DC5269E)
    (at 171 107.5)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5DC52822)
    (attr smd)
    (fp_text reference U4 (at 0 4.3) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value PCM5102A (at 0 -4.3) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -3.75 3.45) (end 2.225 3.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.225 -3.45) (end 2.225 -3.45) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.95 -3.55) (end 3.95 -3.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 3.55) (end 3.95 3.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.95 3.55) (end 3.95 -3.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 3.55) (end -3.95 -3.55) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.2 2.25) (end -1.2 3.25) (layer B.Fab) (width 0.15))
    (fp_line (start -2.2 -3.25) (end -2.2 2.25) (layer B.Fab) (width 0.15))
    (fp_line (start 2.2 -3.25) (end -2.2 -3.25) (layer B.Fab) (width 0.15))
    (fp_line (start 2.2 3.25) (end 2.2 -3.25) (layer B.Fab) (width 0.15))
    (fp_line (start -1.2 3.25) (end 2.2 3.25) (layer B.Fab) (width 0.15))
    (pad 20 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 19 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C10-Pad2)"))
    (pad 17 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 16 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /LRCK))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 /I2SD))
    (pad 13 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /BCLK))
    (pad 12 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(LS2-Pad1)"))
    (pad 6 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(LS1-Pad1)"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 4 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad2)"))
    (pad 3 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C9-Pad1)"))
    (pad 1 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer B.Cu) (tedit 5C97300E) (tstamp 5DC3CFD6)
    (at 59 25 180)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (path /5DC2811A)
    (attr smd)
    (fp_text reference U2 (at 0 6.1) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DS3231M (at 0 -6.1) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 5.93 5.4) (end -5.93 5.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.93 -5.4) (end 5.93 5.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -5.93 -5.4) (end 5.93 -5.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -5.93 5.4) (end -5.93 -5.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.75 4.15) (end -2.75 5.15) (layer B.Fab) (width 0.1))
    (fp_line (start -3.75 -5.15) (end -3.75 4.15) (layer B.Fab) (width 0.1))
    (fp_line (start 3.75 -5.15) (end -3.75 -5.15) (layer B.Fab) (width 0.1))
    (fp_line (start 3.75 5.15) (end 3.75 -5.15) (layer B.Fab) (width 0.1))
    (fp_line (start -2.75 5.15) (end 3.75 5.15) (layer B.Fab) (width 0.1))
    (fp_line (start -3.86 5.005) (end -5.675 5.005) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.86 5.26) (end -3.86 5.005) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 5.26) (end -3.86 5.26) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.86 5.26) (end 3.86 5.005) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 5.26) (end 3.86 5.26) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.86 -5.26) (end -3.86 -5.005) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 -5.26) (end -3.86 -5.26) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.86 -5.26) (end 3.86 -5.005) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 -5.26) (end 3.86 -5.26) (layer B.SilkS) (width 0.12))
    (pad 16 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /SCL))
    (pad 15 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /SDA))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 13 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U2-Pad4)"))
    (pad 3 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U2-Pad3)"))
    (pad 2 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module ESP32-footprints-Lib:ESP32-WROOM (layer B.Cu) (tedit 57D08EA8) (tstamp 5DC52850)
    (at 171 83)
    (path /5DC2247A)
    (fp_text reference U3 (at -11.557 -9.017) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value ESP32-WROOM (at 5.715 -14.224) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -9 -12.75) (end 9 -12.75) (layer B.SilkS) (width 0.15))
    (fp_line (start -9 12.75) (end 9 12.75) (layer B.SilkS) (width 0.15))
    (fp_line (start -9 -12.75) (end -9 12.75) (layer B.SilkS) (width 0.15))
    (fp_line (start 9 -12.75) (end 9 12.75) (layer B.SilkS) (width 0.15))
    (fp_line (start -9 -6.75) (end 9 -6.75) (layer B.SilkS) (width 0.15))
    (fp_text user ESP32-WROOM (at -5.207 -0.254 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 9.906 -6.604) (end 10.033 -6.858) (layer B.SilkS) (width 0.5))
    (fp_text user "Espressif Systems" (at -6.858 0.889 -90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 39 smd rect (at 0.3 2.45) (size 6 6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd oval (at 9 -5.25) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd oval (at 9 -3.98) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 3 smd oval (at 9 -2.71) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /RTS))
    (pad 4 smd oval (at 9 -1.44) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U3-Pad4)"))
    (pad 5 smd oval (at 9 -0.17) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U3-Pad5)"))
    (pad 6 smd oval (at 9 1.1) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U3-Pad6)"))
    (pad 7 smd oval (at 9 2.37) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U3-Pad7)"))
    (pad 8 smd oval (at 9 3.64) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 /LED_DATA))
    (pad 9 smd oval (at 9 4.91) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U3-Pad9)"))
    (pad 10 smd oval (at 9 6.18) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 /LRCK))
    (pad 11 smd oval (at 9 7.45) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 /BCLK))
    (pad 12 smd oval (at 9 8.72) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U3-Pad12)"))
    (pad 13 smd oval (at 9 9.99) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U3-Pad13)"))
    (pad 14 smd oval (at 9 11.26) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U3-Pad14)"))
    (pad 15 smd oval (at 5.715 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd oval (at 4.445 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U3-Pad16)"))
    (pad 17 smd oval (at 3.175 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U3-Pad17)"))
    (pad 18 smd oval (at 1.905 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U3-Pad18)"))
    (pad 19 smd oval (at 0.635 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U3-Pad19)"))
    (pad 20 smd oval (at -0.635 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U3-Pad20)"))
    (pad 21 smd oval (at -1.905 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U3-Pad21)"))
    (pad 22 smd oval (at -3.175 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U3-Pad22)"))
    (pad 23 smd oval (at -4.445 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U3-Pad23)"))
    (pad 24 smd oval (at -5.715 12.75) (size 0.9 2.5) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U3-Pad24)"))
    (pad 25 smd oval (at -9 11.26) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /DTR))
    (pad 26 smd oval (at -9 9.99) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /I2SD))
    (pad 27 smd oval (at -9 8.72) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U3-Pad27)"))
    (pad 28 smd oval (at -9 7.45) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U3-Pad28)"))
    (pad 29 smd oval (at -9 6.18) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 /CS))
    (pad 30 smd oval (at -9 4.91) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 /SCLK))
    (pad 31 smd oval (at -9 3.64) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /MISO))
    (pad 32 smd oval (at -9 2.37) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U3-Pad32)"))
    (pad 33 smd oval (at -9 1.1) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA))
    (pad 34 smd oval (at -9 -0.17) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /RX))
    (pad 35 smd oval (at -9 -1.44) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /TX))
    (pad 36 smd oval (at -9 -2.71) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 17 /SCL))
    (pad 37 smd oval (at -9 -3.98) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 /MOSI))
    (pad 38 smd oval (at -9 -5.25) (size 2.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )

  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD) (tstamp 5DC3CF7C)
    (at 127.7875 24 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /5DC505CD)
    (attr smd)
    (fp_text reference R1 (at 0 1.43) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.43) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
    )
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /RTS))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_Wire:SolderWirePad_1x02_P7.62mm_Drill2.5mm (layer F.Cu) (tedit 5AEE5F2F) (tstamp 5DC40F35)
    (at 183.5 23.5)
    (descr "Wire solder connection")
    (tags connector)
    (path /5DCA1CEC)
    (attr virtual)
    (fp_text reference LS2 (at 3.81 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Speaker (at 3.81 4.445) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.12 3.5) (end -3.5 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.12 3.5) (end 11.12 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -3.5) (end -3.5 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -3.5) (end 11.12 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 7.62 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 11 "Net-(LS2-Pad1)"))
  )

  (module Connector_Wire:SolderWirePad_1x02_P7.62mm_Drill2.5mm (layer F.Cu) (tedit 5AEE5F2F) (tstamp 5DC3CF60)
    (at 89 23.5)
    (descr "Wire solder connection")
    (tags connector)
    (path /5DCA0C56)
    (attr virtual)
    (fp_text reference LS1 (at 3.81 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Speaker (at 3.81 4.445) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.12 3.5) (end -3.5 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.12 3.5) (end 11.12 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -3.5) (end -3.5 3.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -3.5) (end 11.12 -3.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 7.62 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask)
      (net 10 "Net-(LS1-Pad1)"))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB) (tstamp 5DC4180A)
    (at 170.3 18.9 90)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (path /5DC3B538)
    (fp_text reference J2 (at 4.385 2.27 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x05_Male (at 4.385 -12.43 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 2.77 -5.08) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 10.55 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 10.55 -11.95) (end 10.55 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -11.95) (end 10.55 -11.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end -1.8 -11.95) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end 0 1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -10.54) (end 1.44 -10.54) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -9.78) (end 1.44 -9.78) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -10.54) (end 4.1 -10.54) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -9.78) (end 10.1 -10.54) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -9.78) (end 10.1 -9.78) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -8.89) (end 4.1 -8.89) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -8) (end 1.44 -8) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -7.24) (end 1.44 -7.24) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -8) (end 4.1 -8) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -7.24) (end 10.1 -8) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -7.24) (end 10.1 -7.24) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -6.35) (end 4.1 -6.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -5.46) (end 1.44 -5.46) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -4.7) (end 1.44 -4.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -5.46) (end 4.1 -5.46) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -4.7) (end 10.1 -5.46) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -4.7) (end 10.1 -4.7) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -3.81) (end 4.1 -3.81) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -2.92) (end 1.44 -2.92) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.042929 -2.16) (end 1.44 -2.16) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -2.92) (end 4.1 -2.92) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -2.16) (end 10.1 -2.92) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -2.16) (end 10.1 -2.16) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.27) (end 4.1 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.28) (end 10.1 -0.28) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.16) (end 10.1 -0.16) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.04) (end 10.1 -0.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 0.08) (end 10.1 0.08) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 0.2) (end 10.1 0.2) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 0.32) (end 10.1 0.32) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 4.1 -0.38) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 10.1 -0.38) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 0.38) (end 10.1 0.38) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 1.33) (end 1.44 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.1 -11.49) (end 4.1 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 -11.49) (end 4.1 -11.49) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.44 1.33) (end 1.44 -11.49) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.04 -10.48) (end 10.04 -10.48) (layer B.Fab) (width 0.1))
    (fp_line (start 10.04 -9.84) (end 10.04 -10.48) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -9.84) (end 10.04 -9.84) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -10.48) (end 1.5 -10.48) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -9.84) (end -0.32 -10.48) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -9.84) (end 1.5 -9.84) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -7.94) (end 10.04 -7.94) (layer B.Fab) (width 0.1))
    (fp_line (start 10.04 -7.3) (end 10.04 -7.94) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -7.3) (end 10.04 -7.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -7.94) (end 1.5 -7.94) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -7.3) (end -0.32 -7.94) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -7.3) (end 1.5 -7.3) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -5.4) (end 10.04 -5.4) (layer B.Fab) (width 0.1))
    (fp_line (start 10.04 -4.76) (end 10.04 -5.4) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -4.76) (end 10.04 -4.76) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -5.4) (end 1.5 -5.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -4.76) (end -0.32 -5.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -4.76) (end 1.5 -4.76) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -2.86) (end 10.04 -2.86) (layer B.Fab) (width 0.1))
    (fp_line (start 10.04 -2.22) (end 10.04 -2.86) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -2.22) (end 10.04 -2.22) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -2.86) (end 1.5 -2.86) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -2.22) (end -0.32 -2.86) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -2.22) (end 1.5 -2.22) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer B.Fab) (width 0.1))
    (fp_line (start 10.04 0.32) (end 10.04 -0.32) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end -0.32 -0.32) (layer B.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 0.635) (end 2.135 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.5 -11.43) (end 1.5 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 -11.43) (end 1.5 -11.43) (layer B.Fab) (width 0.1))
    (fp_line (start 4.04 1.27) (end 4.04 -11.43) (layer B.Fab) (width 0.1))
    (fp_line (start 2.135 1.27) (end 4.04 1.27) (layer B.Fab) (width 0.1))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DTR))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /TX))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RX))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /RTS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A) (tstamp 5DC3CEFB)
    (at 21 60 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5DC2448B)
    (fp_text reference J1 (at -8.45 5.75 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -3.75) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.05 -4.8) (end 1.1 -4.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.1 -3.75) (end 1.1 -4.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.003213 -4.505425) (end 0.8 -3.75) (layer F.Fab) (width 0.1))
    (fp_text user %R (at -3 -2.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 3 thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC3CED8)
    (at 68 41.2125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DC4CCEA)
    (attr smd)
    (fp_text reference C4 (at 0 1.43 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 4.7u (at 0 -1.43 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
    )
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC3CEC7)
    (at 50.5 41.2875 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DC4B9FA)
    (attr smd)
    (fp_text reference C3 (at 0 1.43 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 4.7u (at 0 -1.43 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)) (justify mirror))
    )
    (fp_line (start 1.48 -0.73) (end -1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end 1.48 -0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 0.73) (end 1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end -1.48 0.73) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC43014)
    (at 178.5 108.515 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DCA89C8)
    (attr smd)
    (fp_text reference C10 (at 0 1.17 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -1.17 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C10-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC42FEA)
    (at 164 108.985 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DCA2377)
    (attr smd)
    (fp_text reference C9 (at 0 1.17 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 2.2u (at 0 -1.17 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C9-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC42FC0)
    (at 164 106.515 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DCC0191)
    (attr smd)
    (fp_text reference C11 (at 0 1.17 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 2.2u (at 0 -1.17 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer B.Cu) (tedit 5AE50EF0) (tstamp 5DC3CE89)
    (at 20 68 180)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (path /5DC5A769)
    (fp_text reference C2 (at 1.75 5.25) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1m (at 1.75 -5.25) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 1.75 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.259698 2.715) (end -2.259698 1.915) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.659698 2.315) (end -1.859698 2.315) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.831 0.533) (end 5.831 -0.533) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.791 0.768) (end 5.791 -0.768) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.751 0.948) (end 5.751 -0.948) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.711 1.098) (end 5.711 -1.098) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.671 1.229) (end 5.671 -1.229) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.631 1.346) (end 5.631 -1.346) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.591 1.453) (end 5.591 -1.453) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.551 1.552) (end 5.551 -1.552) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.511 1.645) (end 5.511 -1.645) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.471 1.731) (end 5.471 -1.731) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.431 1.813) (end 5.431 -1.813) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.391 1.89) (end 5.391 -1.89) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.351 1.964) (end 5.351 -1.964) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.311 2.034) (end 5.311 -2.034) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.271 2.102) (end 5.271 -2.102) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.231 2.166) (end 5.231 -2.166) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.191 2.228) (end 5.191 -2.228) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.151 2.287) (end 5.151 -2.287) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.111 2.345) (end 5.111 -2.345) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.071 2.4) (end 5.071 -2.4) (layer B.SilkS) (width 0.12))
    (fp_line (start 5.031 2.454) (end 5.031 -2.454) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.991 2.505) (end 4.991 -2.505) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.951 2.556) (end 4.951 -2.556) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.911 2.604) (end 4.911 -2.604) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.871 2.651) (end 4.871 -2.651) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.831 2.697) (end 4.831 -2.697) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.791 2.741) (end 4.791 -2.741) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.751 2.784) (end 4.751 -2.784) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.711 2.826) (end 4.711 -2.826) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.671 2.867) (end 4.671 -2.867) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.631 2.907) (end 4.631 -2.907) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.591 2.945) (end 4.591 -2.945) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.551 2.983) (end 4.551 -2.983) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.511 -1.04) (end 4.511 -3.019) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.511 3.019) (end 4.511 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.471 -1.04) (end 4.471 -3.055) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.471 3.055) (end 4.471 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.431 -1.04) (end 4.431 -3.09) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.431 3.09) (end 4.431 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.391 -1.04) (end 4.391 -3.124) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.391 3.124) (end 4.391 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.351 -1.04) (end 4.351 -3.156) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.351 3.156) (end 4.351 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.311 -1.04) (end 4.311 -3.189) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.311 3.189) (end 4.311 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.271 -1.04) (end 4.271 -3.22) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.271 3.22) (end 4.271 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.231 -1.04) (end 4.231 -3.25) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.231 3.25) (end 4.231 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.191 -1.04) (end 4.191 -3.28) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.191 3.28) (end 4.191 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.151 -1.04) (end 4.151 -3.309) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.151 3.309) (end 4.151 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.111 -1.04) (end 4.111 -3.338) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.111 3.338) (end 4.111 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.071 -1.04) (end 4.071 -3.365) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.071 3.365) (end 4.071 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.031 -1.04) (end 4.031 -3.392) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.031 3.392) (end 4.031 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.991 -1.04) (end 3.991 -3.418) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.991 3.418) (end 3.991 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.951 -1.04) (end 3.951 -3.444) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.951 3.444) (end 3.951 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.911 -1.04) (end 3.911 -3.469) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.911 3.469) (end 3.911 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.871 -1.04) (end 3.871 -3.493) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.871 3.493) (end 3.871 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.831 -1.04) (end 3.831 -3.517) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.831 3.517) (end 3.831 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.791 -1.04) (end 3.791 -3.54) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.791 3.54) (end 3.791 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.751 -1.04) (end 3.751 -3.562) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.751 3.562) (end 3.751 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.711 -1.04) (end 3.711 -3.584) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.711 3.584) (end 3.711 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.671 -1.04) (end 3.671 -3.606) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.671 3.606) (end 3.671 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.631 -1.04) (end 3.631 -3.627) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.631 3.627) (end 3.631 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.591 -1.04) (end 3.591 -3.647) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.591 3.647) (end 3.591 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.551 -1.04) (end 3.551 -3.666) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.551 3.666) (end 3.551 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.511 -1.04) (end 3.511 -3.686) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.511 3.686) (end 3.511 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.471 -1.04) (end 3.471 -3.704) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.471 3.704) (end 3.471 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.431 -1.04) (end 3.431 -3.722) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.431 3.722) (end 3.431 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.391 -1.04) (end 3.391 -3.74) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.391 3.74) (end 3.391 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.351 -1.04) (end 3.351 -3.757) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.351 3.757) (end 3.351 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.311 -1.04) (end 3.311 -3.774) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.311 3.774) (end 3.311 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.271 -1.04) (end 3.271 -3.79) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.271 3.79) (end 3.271 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.231 -1.04) (end 3.231 -3.805) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.231 3.805) (end 3.231 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.191 -1.04) (end 3.191 -3.821) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.191 3.821) (end 3.191 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.151 -1.04) (end 3.151 -3.835) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.151 3.835) (end 3.151 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.111 -1.04) (end 3.111 -3.85) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.111 3.85) (end 3.111 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.071 -1.04) (end 3.071 -3.863) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.071 3.863) (end 3.071 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.031 -1.04) (end 3.031 -3.877) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.031 3.877) (end 3.031 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.991 -1.04) (end 2.991 -3.889) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.991 3.889) (end 2.991 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.951 -1.04) (end 2.951 -3.902) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.951 3.902) (end 2.951 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.911 -1.04) (end 2.911 -3.914) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.911 3.914) (end 2.911 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.871 -1.04) (end 2.871 -3.925) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.871 3.925) (end 2.871 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.831 -1.04) (end 2.831 -3.936) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.831 3.936) (end 2.831 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.791 -1.04) (end 2.791 -3.947) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.791 3.947) (end 2.791 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.751 -1.04) (end 2.751 -3.957) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.751 3.957) (end 2.751 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.711 -1.04) (end 2.711 -3.967) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.711 3.967) (end 2.711 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.671 -1.04) (end 2.671 -3.976) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.671 3.976) (end 2.671 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.631 -1.04) (end 2.631 -3.985) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.631 3.985) (end 2.631 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.591 -1.04) (end 2.591 -3.994) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.591 3.994) (end 2.591 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.551 -1.04) (end 2.551 -4.002) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.551 4.002) (end 2.551 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.511 -1.04) (end 2.511 -4.01) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.511 4.01) (end 2.511 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.471 -1.04) (end 2.471 -4.017) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.471 4.017) (end 2.471 1.04) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.43 4.024) (end 2.43 -4.024) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.39 4.03) (end 2.39 -4.03) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.35 4.037) (end 2.35 -4.037) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.31 4.042) (end 2.31 -4.042) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.27 4.048) (end 2.27 -4.048) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.23 4.052) (end 2.23 -4.052) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.19 4.057) (end 2.19 -4.057) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.15 4.061) (end 2.15 -4.061) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.11 4.065) (end 2.11 -4.065) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.07 4.068) (end 2.07 -4.068) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.03 4.071) (end 2.03 -4.071) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.99 4.074) (end 1.99 -4.074) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.95 4.076) (end 1.95 -4.076) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.91 4.077) (end 1.91 -4.077) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.87 4.079) (end 1.87 -4.079) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.83 4.08) (end 1.83 -4.08) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.79 4.08) (end 1.79 -4.08) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 4.08) (end 1.75 -4.08) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.276759 2.1475) (end -1.276759 1.3475) (layer B.Fab) (width 0.1))
    (fp_line (start -1.676759 1.7475) (end -0.876759 1.7475) (layer B.Fab) (width 0.1))
    (fp_circle (center 1.75 0) (end 6 0) (layer B.CrtYd) (width 0.05))
    (fp_circle (center 1.75 0) (end 5.87 0) (layer B.SilkS) (width 0.12))
    (fp_circle (center 1.75 0) (end 5.75 0) (layer B.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC42F96)
    (at 181 110.015 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DCAD956)
    (attr smd)
    (fp_text reference C8 (at 0 1.17 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -1.17 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_Elec_8x10.2 (layer B.Cu) (tedit 5BC8D926) (tstamp 5DC5297D)
    (at 32 57 90)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 8.0x10.2mm")
    (tags "capacitor electrolyic nonpolar")
    (path /5DC5A0AA)
    (attr smd)
    (fp_text reference C1 (at 0 5.2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1m (at 0 -5.2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -6.1 -1.3) (end -4.4 -1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -6.1 1.3) (end -6.1 -1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 1.3) (end -6.1 1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 -1.3) (end -4.4 -3.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 3.25) (end -4.4 1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 3.25) (end -3.25 4.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.4 -3.25) (end -3.25 -4.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.25 4.4) (end 4.4 4.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.25 -4.4) (end 4.4 -4.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.4 -1.3) (end 4.4 -4.4) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6.1 -1.3) (end 4.4 -1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start 6.1 1.3) (end 6.1 -1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.4 1.3) (end 6.1 1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start 4.4 4.4) (end 4.4 1.3) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.26 -3.195563) (end -3.195563 -4.26) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.26 3.195563) (end -3.195563 4.26) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.26 3.195563) (end -4.26 1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.26 -3.195563) (end -4.26 -1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.195563 -4.26) (end 4.26 -4.26) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.195563 4.26) (end 4.26 4.26) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.26 4.26) (end 4.26 1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.26 -4.26) (end 4.26 -1.31) (layer B.SilkS) (width 0.12))
    (fp_line (start -4.15 -3.15) (end -3.15 -4.15) (layer B.Fab) (width 0.1))
    (fp_line (start -4.15 3.15) (end -3.15 4.15) (layer B.Fab) (width 0.1))
    (fp_line (start -4.15 3.15) (end -4.15 -3.15) (layer B.Fab) (width 0.1))
    (fp_line (start -3.15 -4.15) (end 4.15 -4.15) (layer B.Fab) (width 0.1))
    (fp_line (start -3.15 4.15) (end 4.15 4.15) (layer B.Fab) (width 0.1))
    (fp_line (start 4.15 4.15) (end 4.15 -4.15) (layer B.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 4 0) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 3.6 0 90) (size 4.5 2.1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.119048)
      (net 1 GND))
    (pad 1 smd roundrect (at -3.6 0 90) (size 4.5 2.1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.119048)
      (net 5 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_Elec_8x10.2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC3CDAD)
    (at 129 19.515 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DC37A96)
    (attr smd)
    (fp_text reference C6 (at 0 1.17 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -1.17 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC3CD9E)
    (at 126.5 19.485 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DC36963)
    (attr smd)
    (fp_text reference C5 (at 0 1.17 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -1.17 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE) (tstamp 5DC3CD8F)
    (at 124 23.515 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /5DC4EC03)
    (attr smd)
    (fp_text reference C7 (at 0 1.17 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100n (at 0 -1.17 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.25 0.25) (thickness 0.04)) (justify mirror))
    )
    (fp_line (start 0.93 -0.47) (end -0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.93 0.47) (end 0.93 -0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 0.47) (end 0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.93 -0.47) (end -0.93 0.47) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.5 -0.25) (end -0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end 0.5 -0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end 0.5 0.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end -0.5 0.25) (layer B.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 /RTS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Battery:BatteryHolder_Keystone_1058_1x2032 (layer B.Cu) (tedit 589EE147) (tstamp 5DC41534)
    (at 38.4 34.08 90)
    (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
    (tags "Keystone type 1058 coin cell retainer")
    (path /5DC29E69)
    (attr smd)
    (fp_text reference BT1 (at 0 -7.62 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Battery_Cell (at 0 9.398 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_circle (center 0 0) (end 10 0) (layer Dwgs.User) (width 0.15))
    (fp_arc (start 0 0) (end -10.61275 3.5) (angle -27.4635) (layer B.Fab) (width 0.1))
    (fp_line (start -7.8026 8) (end 7.8026 8) (layer B.Fab) (width 0.1))
    (fp_line (start -3.9 -8) (end -7.8026 -8) (layer B.Fab) (width 0.1))
    (fp_line (start -14.2 3.5) (end -14.2 1.9) (layer B.Fab) (width 0.1))
    (fp_line (start -14.2 3.5) (end -10.61275 3.5) (layer B.Fab) (width 0.1))
    (fp_line (start -1.7 -5.8) (end 1.7 -5.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.7 -5.8) (end -3.9 -8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.7 -5.8) (end 3.9 -8) (layer B.Fab) (width 0.1))
    (fp_line (start 3.9 -8) (end 7.8026 -8) (layer B.Fab) (width 0.1))
    (fp_line (start -14.2 -3.5) (end -10.61275 -3.5) (layer B.Fab) (width 0.1))
    (fp_line (start -14.2 -1.9) (end -14.2 -3.5) (layer B.Fab) (width 0.1))
    (fp_line (start 14.2 3.5) (end 14.2 1.9) (layer B.Fab) (width 0.1))
    (fp_line (start 10.61275 3.5) (end 14.2 3.5) (layer B.Fab) (width 0.1))
    (fp_line (start 14.2 -3.5) (end 10.61275 -3.5) (layer B.Fab) (width 0.1))
    (fp_line (start 14.2 -1.9) (end 14.2 -3.5) (layer B.Fab) (width 0.1))
    (fp_arc (start 0 0) (end 10.61275 -3.5) (angle -27.4635) (layer B.Fab) (width 0.1))
    (fp_arc (start 0 0) (end 10.61275 3.5) (angle 27.4635) (layer B.Fab) (width 0.1))
    (fp_arc (start 0 0) (end -10.61275 -3.5) (angle 27.4635) (layer B.Fab) (width 0.1))
    (fp_line (start -14.31 3.61) (end -10.692 3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start -14.31 1.9) (end -14.31 3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start -7.8473 8.11) (end 7.8473 8.11) (layer B.SilkS) (width 0.12))
    (fp_line (start 14.31 1.9) (end 14.31 3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 10.692 3.61) (end 14.31 3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 14.31 -3.61) (end 10.692 -3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 14.31 -1.9) (end 14.31 -3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start 7.8473 -8.11) (end 3.86 -8.11) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.66 -5.91) (end 3.86 -8.11) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.66 -5.91) (end -1.66 -5.91) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.66 -5.91) (end -3.86 -8.11) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.86 -8.11) (end -7.8473 -8.11) (layer B.SilkS) (width 0.12))
    (fp_line (start -10.692 -3.61) (end -14.31 -3.61) (layer B.SilkS) (width 0.12))
    (fp_line (start -14.31 -1.9) (end -14.31 -3.61) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0 0) (end -10.692 3.61) (angle -27.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0 0) (end 10.692 -3.61) (angle -27.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0 0) (end 10.692 3.61) (angle 27.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0 0) (end -10.692 -3.61) (angle 27.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -16.45 -4.11) (end -11.06 -4.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -16.45 4.11) (end -16.45 -4.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -16.45 4.11) (end -11.06 4.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start 16.45 4.11) (end 11.06 4.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start 16.45 -4.11) (end 16.45 4.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start 11.06 -4.11) (end 16.45 -4.11) (layer B.CrtYd) (width 0.05))
    (fp_arc (start 0 0) (end -11.06 4.11) (angle -139.2) (layer B.CrtYd) (width 0.05))
    (fp_arc (start 0 0) (end 11.06 -4.11) (angle -139.2) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 14.68 0 90) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -14.68 0 90) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1058_1x2032.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
