(module ESP32-WROOM (layer F.Cu) (tedit 57D08EA8)
  (fp_text reference REF** (at -11.557 9.017) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ESP32-WROOM (at 5.715 14.224) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Espressif Systems" (at -6.858 -0.889 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 9.906 6.604) (end 10.033 6.858) (layer F.SilkS) (width 0.5))
  (fp_text user ESP32-WROOM (at -5.207 0.254 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9 6.75) (end 9 6.75) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 12.75) (end 9 -12.75) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 12.75) (end -9 -12.75) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 -12.75) (end 9 -12.75) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 12.75) (end 9 12.75) (layer F.SilkS) (width 0.15))
  (pad 38 smd oval (at -9 5.25) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd oval (at -9 3.98) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd oval (at -9 2.71) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd oval (at -9 1.44) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd oval (at -9 0.17) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd oval (at -9 -1.1) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd oval (at -9 -2.37) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd oval (at -9 -3.64) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd oval (at -9 -4.91) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd oval (at -9 -6.18) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd oval (at -9 -7.45) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd oval (at -9 -8.72) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd oval (at -9 -9.99) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd oval (at -9 -11.26) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at -5.715 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at -4.445 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at -3.175 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at -1.905 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at -0.635 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 0.635 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 1.905 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 3.175 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at 4.445 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 5.715 -12.75) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 9 -11.26) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 9 -9.99) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 9 -8.72) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 9 -7.45) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 9 -6.18) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 9 -4.91) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 9 -3.64) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 9 -2.37) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 9 -1.1) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at 9 0.17) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at 9 1.44) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at 9 2.71) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at 9 3.98) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd oval (at 9 5.25) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 0.3 -2.45) (size 6 6) (layers F.Cu F.Paste F.Mask))
)
