(footprint "ESP32-S3-DevKitC" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 635FDFCD)
  (descr "ESP32-S3 general-purpose development board, based on ESP32-S3-WROOM-1 or ESP32-S3-WROOM-1U,It has all the ESP32-S3 pins exposed and is easy to connect and use.")
  (tags "ESP32-S3")
  (attr through_hole)
  (fp_text reference "REF**" (at 12.7 -2.1) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c8227f23-f85b-4d5e-b1ca-65f8823f3974)
  )
  (fp_text value "ESP32-S3-DevKitC" (at 11.42632 29.46128 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0ab80b09-6a1d-4c02-8228-6d216fd37b48)
  )
  (fp_text user "3V3" (at 1.27 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 02948ab8-efee-4b6f-b1c3-8f2856a81885)
  )
  (fp_text user "GPIO37" (at 21.59 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 0961119e-2c3e-453d-b7a3-bcff9d1a7e21)
  )
  (fp_text user "GND" (at 1.52032 53.33728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 09cabdf7-e482-45d5-8508-f0848474bb1f)
  )
  (fp_text user "GPIO21" (at 21.59 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 09df8f63-15ca-46e7-bd53-89e1a452b90e)
  )
  (fp_text user "GPIO4" (at 1.27 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 0a70bd0b-36c5-4375-bf1e-bbb10c87148e)
  )
  (fp_text user "GPIO13" (at 1.27 45.72 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 1b941ef5-5418-4751-9ec4-03dd20cb8de6)
  )
  (fp_text user "GPIO5" (at 1.27 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 1be8d931-dd9f-4b2b-96b1-b581f52a754f)
  )
  (fp_text user "GPIO19" (at 21.59 48.26 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 20df80e6-7b97-49d7-8b48-f83e7540d820)
  )
  (fp_text user "GPIO9" (at 1.27 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 27c951eb-87bf-4f1c-9dfa-59996eee12e3)
  )
  (fp_text user "GPIO47" (at 21.59 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 36672a27-89ae-4033-9152-995fb3afa0e9)
  )
  (fp_text user "GPIO14" (at 1.27 48.26 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 40abb8eb-7c16-4e45-99dc-6ef5b0075487)
  )
  (fp_text user "GPIO40/MTDO" (at 21.59 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 46a31786-b55a-49da-9e08-f225bcb6cf76)
  )
  (fp_text user "GPIO7" (at 1.27 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 4bda75b3-eace-41b3-80c4-c44588ca34cf)
  )
  (fp_text user "GPIO11" (at 1.27 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 4ecaf681-48bc-4755-b366-740204c042c1)
  )
  (fp_text user "GPIO46" (at 1.27 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 5444ff6f-fbb1-4f38-94fe-5eada818d583)
  )
  (fp_text user "GPIO12" (at 1.27 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 5ed1fff4-ce0c-454c-b5fe-3fd95080ebd2)
  )
  (fp_text user "GPIO17" (at 1.27 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 6e5db457-c7f8-4d06-87e8-dd96cc4c1214)
  )
  (fp_text user "EN/RESET" (at 8.88632 5.07728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 70695e4b-e845-4e99-a841-5cc37a0df072)
  )
  (fp_text user "GPIO48" (at 21.59 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 7626a14d-29b7-4a07-bae9-7f7a3c14fbd0)
  )
  (fp_text user "GPIO41/MTDI" (at 21.59 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 77b57aac-a1eb-4734-88cd-9d0647bd6382)
  )
  (fp_text user "GND" (at 21.59 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 7f6ac43c-67c4-4f98-8e25-cc5d46641e4d)
  )
  (fp_text user "GPIO35" (at 21.59 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 811b6bf1-e333-4685-ae04-082f6afcc4e6)
  )
  (fp_text user "GPIO6" (at 1.27 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 84be3903-7a00-42c7-943e-8ed422e01557)
  )
  (fp_text user "GPIO39/MTCK" (at 21.59 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 9c6f8f01-1b36-4681-a7db-1edda8289ebf)
  )
  (fp_text user "GPIO8" (at 1.27 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b16f2d5d-1099-4a97-9142-35b5248315bf)
  )
  (fp_text user "GPIO1" (at 21.59 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp b71e5bb7-6d4d-4b68-b6a9-2816f916640f)
  )
  (fp_text user "GPIO44/U0RXD" (at 21.59 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp b7c364bd-04fd-4610-87e9-ccc02cc8da16)
  )
  (fp_text user "GND" (at 21.59 53.34 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp ba3986f5-0209-45b3-8bb5-249a033f03b0)
  )
  (fp_text user "5V" (at 1.52032 50.79728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp bb012883-526e-4f29-9d5b-7f95e23e0b19)
  )
  (fp_text user "GPIO18" (at 1.27 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp bb7d3d72-93cd-4ac7-8df5-3db3b91b2853)
  )
  (fp_text user "GPIO20" (at 21.59 45.72 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp c0d42894-b37b-4d54-9002-e4cc5b6af2a4)
  )
  (fp_text user "3V3" (at 1.27 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp c974b321-5c82-4530-ac33-56d04589f4ea)
  )
  (fp_text user "GPIO42/MTMS" (at 21.59 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp cb42479f-d7b0-4a96-9926-f81c8038c50c)
  )
  (fp_text user "GPIO15" (at 1.27 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp cfffd01e-4c1d-46e1-a18b-4d2817930aac)
  )
  (fp_text user "GND" (at 21.59 50.8 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp d8f38a58-42dc-4ba2-9b36-8f484b567900)
  )
  (fp_text user "GPIO0" (at 21.59 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp dbf44227-af21-41bd-bc2d-28a959c548fb)
  )
  (fp_text user "GPIO2" (at 21.59 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp dd14a8fb-ae12-45ee-a3ae-20ac0ecdf4ab)
  )
  (fp_text user "GPIO43/U0TXD" (at 21.59 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp e2019170-a35d-4646-878c-a7e30159e571)
  )
  (fp_text user "GPIO16" (at 1.27 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e48a2571-0142-4fe0-91a1-90feecb7745f)
  )
  (fp_text user "GPIO45" (at 21.59 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp ea833c0d-5cde-4cb2-85ef-860c83cdb0ff)
  )
  (fp_text user "GPIO3" (at 1.27 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp f0240cd6-ef06-4386-82aa-f38f9d200ce9)
  )
  (fp_text user "GPIO38" (at 21.59 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp f269c0b8-3865-431e-9599-a4f3bd5e81c7)
  )
  (fp_text user "GPIO36" (at 21.59 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp fa29d936-9fc8-4db7-86f3-d9ae67708e2d)
  )
  (fp_text user "GPIO10" (at 1.27 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp fe978faa-5402-4b2d-8b3d-a3d9f14f427a)
  )
  (fp_text user "REF**" (at -0.00368 -0.00272) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bb817733-2b63-4d0b-b6f5-207f34e5db94)
  )
  (fp_line (start -1.5 62.79728) (end 24.359999 62.79728) (layer "F.SilkS") (width 0.12) (tstamp 3be6995c-1b5d-4206-a779-77dd7d4dfea4))
  (fp_line (start 24.36 -1.1) (end -1.499999 -1.1) (layer "F.SilkS") (width 0.12) (tstamp 4cf41fbf-09c6-45d2-a08a-a6e86d4fe57e))
  (fp_line (start 24.359999 62.79728) (end 24.36 -1.1) (layer "F.SilkS") (width 0.12) (tstamp 547dba7f-4c60-495a-9cbc-7940c573b812))
  (fp_line (start -1.499999 -1.1) (end -1.5 62.79728) (layer "F.SilkS") (width 0.12) (tstamp 9a426851-f9e8-488e-843e-2714cd380a03))
  (fp_line (start 2.46012 -7.01312) (end 20.44332 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp a7220907-a9f0-478a-b770-221830a56666))
  (fp_line (start 20.44332 -7.01312) (end 20.44332 -1.12032) (layer "F.SilkS") (width 0.12) (tstamp b1c9279b-fe2f-4e7c-9260-71ab486e55f0))
  (fp_line (start 2.46012 -1.12032) (end 2.46012 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp c496ba81-d915-4830-89f0-5ee328f829b6))
  (fp_line (start -1.25 -0.85) (end 24.11 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 5079bec5-7960-47f5-bb2a-838d62f09a10))
  (fp_line (start -1.25 62.54728) (end -1.25 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 700f1d52-3495-4ce1-a67a-8ed4bd4d89d9))
  (fp_line (start 24.11 62.54728) (end -1.25 62.54728) (layer "F.CrtYd") (width 0.05) (tstamp bd47c505-732e-4cbb-b5ee-95917ddebf97))
  (fp_line (start 24.11 -0.85) (end 24.11 62.54728) (layer "F.CrtYd") (width 0.05) (tstamp f7a594c2-a1e0-4a31-9261-1a2ff29fe96a))
  (pad "1" thru_hole rect (at 0 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c853012e-700f-4da9-9452-f9fe0ab21c4a))
  (pad "2" thru_hole oval (at 0 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d1d01c2e-a6b6-404d-9fdd-e80e028ca1be))
  (pad "3" thru_hole oval (at 0 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ccc491e7-9251-422d-80e0-7ad308cc5972))
  (pad "4" thru_hole oval (at 0 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e1bf0850-7ec6-401b-b7d2-ca77a5ee24f2))
  (pad "5" thru_hole oval (at 0 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 739a5348-0378-48de-8d71-542a3da55545))
  (pad "6" thru_hole oval (at 0 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b0c6867f-27f0-4d8b-8de1-ac0c8b68d518))
  (pad "7" thru_hole oval (at 0 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 95426ea0-b124-4683-83d4-dd9a448d6175))
  (pad "8" thru_hole oval (at 0 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 56b22375-2da3-43ef-b7d3-f0b423ba7f3b))
  (pad "9" thru_hole oval (at 0 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ec3a1345-f14d-407f-b544-d0b28d52f485))
  (pad "10" thru_hole oval (at 0 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 13630c47-b459-4961-a710-9cf7d93cdb56))
  (pad "11" thru_hole oval (at 0 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 12e1753d-bf94-4be5-88d4-b5c37757ca74))
  (pad "12" thru_hole oval (at 0 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 986568c5-5610-4782-91a3-f8e10ff8db02))
  (pad "13" thru_hole oval (at 0 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c04e69df-fbc5-4c87-9f99-51cc8a8fce4f))
  (pad "14" thru_hole oval (at 0 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6b14c8db-d2bb-464d-b050-6422db4e6acb))
  (pad "15" thru_hole oval (at 0 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b0374586-2bc8-434f-9bcb-b3f54b4a89cc))
  (pad "16" thru_hole oval (at 0 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d3bc05fd-f3fd-477a-8f87-ab5e668d627a))
  (pad "17" thru_hole oval (at 0 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 44321113-af3a-4d9e-bf31-d2770c836e5e))
  (pad "18" thru_hole oval (at 0 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 4a443588-6a1d-408e-a939-f58fed09f5ca))
  (pad "19" thru_hole oval (at 0 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp aa0681ca-f686-4a61-a1ef-4dec48518b40))
  (pad "20" thru_hole oval (at -0.00368 48.25728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp eee343b0-95fe-4edf-95bc-253d7c264814))
  (pad "21" thru_hole oval (at -0.00368 50.79728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 682e5757-74d8-4566-941f-5c2dc4b08861))
  (pad "22" thru_hole oval (at -0.00368 53.33728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0a358951-dc0f-455f-b40e-a448a2d62296))
  (pad "23" thru_hole oval (at 22.86 53.34 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 2ce747d2-6867-415e-ad62-07d955f55c7d))
  (pad "24" thru_hole oval (at 22.86 50.8 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 9c465851-4b43-4b71-8924-73a99f165718))
  (pad "25" thru_hole oval (at 22.86 48.26 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 550f05da-7829-4e54-8ee0-6bdeaafcbd8a))
  (pad "26" thru_hole oval (at 22.86 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 78257f4a-280b-40c6-bfcd-1a927e7af789))
  (pad "27" thru_hole oval (at 22.86 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp cb770979-c6fc-45d5-9ee2-fef7c1168fba))
  (pad "28" thru_hole oval (at 22.86 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 2e3350ad-e61a-42d1-857c-c6b31e00a397))
  (pad "29" thru_hole oval (at 22.86 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d0dae0f9-8a88-4ef1-9511-18529adba88a))
  (pad "30" thru_hole oval (at 22.86 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 767d6240-4ee5-48a7-98b3-5cb707b449cb))
  (pad "31" thru_hole oval (at 22.86 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp a60f7623-e638-4072-8099-ba86a12ecc89))
  (pad "32" thru_hole oval (at 22.86 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp f2d85f0b-cd4c-4e62-a8f6-7433cb5a7c23))
  (pad "33" thru_hole oval (at 22.86 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 25fa8036-8b5e-4bc0-b4cd-f4c726cf3d62))
  (pad "34" thru_hole oval (at 22.86 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c40456a7-b09c-40b8-b35f-246e0f09c1f0))
  (pad "35" thru_hole oval (at 22.86 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6f6d496b-6b03-4b31-be82-29446a572c31))
  (pad "36" thru_hole oval (at 22.86 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c120d961-bf26-4a15-912e-9d7e57ef4081))
  (pad "37" thru_hole oval (at 22.86 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 7231f57f-8d8d-419c-a764-9c9a9a6ebbda))
  (pad "38" thru_hole oval (at 22.86 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c9b89280-b75e-41b6-9c3d-8ff6ee2b8db6))
  (pad "39" thru_hole oval (at 22.86 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 3eb34af4-da13-4e59-8401-9125bfa36c5b))
  (pad "40" thru_hole oval (at 22.86 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 84bb6cb8-2f9e-4287-adf5-04288da39e8d))
  (pad "41" thru_hole oval (at 22.86 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b7e8be93-a8c9-4176-8ef1-ddcd285b23cb))
  (pad "42" thru_hole oval (at 22.86 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 84580140-034f-4289-8e39-fb2aa8629d7c))
  (pad "43" thru_hole oval (at 22.86 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp adb9fa15-0d86-4be7-9faf-5c0be8715635))
  (pad "44" thru_hole oval (at 22.86 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 04b3d92e-122f-4322-a4b6-c536a6e4dae8))
)
