(footprint "ESP32-DevKitC" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 635FD713)
  (descr "ESP32-DevKitC: https://docs.espressif.com/projects/esp-idf/en/latest/esp32/hw-reference/esp32/get-started-devkitc.html")
  (tags "ESP32")
  (attr through_hole)
  (fp_text reference "REF**" (at 12.7 -2.1) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d18878b3-3936-41f9-899c-b145c0e75657)
  )
  (fp_text value "ESP32-DevKitC" (at 12.7 24.13 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0abccbfb-c01a-4118-bd1b-13b6bbb78c24)
  )
  (fp_text user "D1" (at 24.13 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 07ea5560-c845-4753-893d-0f7876dceabc)
  )
  (fp_text user "GPIO2" (at 24.13 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 0ada659b-c675-4427-90ca-f67dcc4b7779)
  )
  (fp_text user "VN/GPIO39" (at 1.27 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 0de0b64b-b090-4327-890e-18f8dfd50b93)
  )
  (fp_text user "GPIO13/MTCK" (at 1.27 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 1da192c9-d020-43d3-9638-e8a1dd9256f4)
  )
  (fp_text user "GPIO22" (at 24.13 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 23aa612d-350a-47d6-b49d-082baeb19226)
  )
  (fp_text user "GND" (at 1.27 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 2be119c6-674a-4203-b30c-fc431d0af933)
  )
  (fp_text user "GPIO32" (at 1.27 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 3149690b-401f-4f0f-a106-d4a9758653eb)
  )
  (fp_text user "GPIO1/U0TXD" (at 24.13 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 383063a8-a62d-4ec0-a6b3-7810dce07992)
  )
  (fp_text user "D2" (at 1.27 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 3c339ed2-1113-418a-afc9-d9e1ab0d2a52)
  )
  (fp_text user "GND" (at 24.13 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 3d439381-bbbf-4d40-84d0-2247abcc01d2)
  )
  (fp_text user "3V3" (at 1.27 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 3dd13f9c-ffc7-409b-b096-a3014ce942a9)
  )
  (fp_text user "GND" (at 24.13 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 3ee35c0c-be4a-438e-81f5-46ded4529810)
  )
  (fp_text user "GPIO15/MTDO" (at 24.13 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 42c7b515-a1ec-40ad-a41f-5b3478e22ece)
  )
  (fp_text user "GPIO19" (at 24.13 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 42c8b4b6-47a7-45e9-a86c-e6710f599a08)
  )
  (fp_text user "GPIO35" (at 1.27 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 4b2b15a0-55ff-4e43-86e8-289c7715a987)
  )
  (fp_text user "EN/RESET" (at 8.88632 2.53728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 54ae2335-8a6a-4054-a846-03c9ad1638cd)
  )
  (fp_text user "VP/GPIO36" (at 1.27 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 6289a9d0-a3d1-4bea-842b-95db0a7ccccd)
  )
  (fp_text user "GPIO17" (at 24.13 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 64e10da7-ccab-407f-be35-6875f09012f7)
  )
  (fp_text user "GPIO25" (at 1.27 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 6bc4d1df-c71b-4534-a4d1-a1edc9f00ba7)
  )
  (fp_text user "GPIO16" (at 24.13 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 6c677598-7972-4eeb-9443-f04338aefc71)
  )
  (fp_text user "5V" (at 1.26632 45.97128 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 6daeb035-12ad-4e9f-9947-2ae236e7cfaa)
  )
  (fp_text user "GPIO34" (at 1.27 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 6e0bdcc9-dacd-4322-ae59-de64405a14cc)
  )
  (fp_text user "GPIO33" (at 1.27 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 85b96d91-db7a-4de7-b32d-f36ef8d92fbc)
  )
  (fp_text user "GPIO4" (at 24.13 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 86757deb-d9f1-4627-abbe-76b99ccff3b6)
  )
  (fp_text user "GPIO5" (at 24.13 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 89bfd096-79ba-4e98-8c2b-e2ecb5eb62ed)
  )
  (fp_text user "GPIO27" (at 1.27 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 8d2e0e54-2cbd-495a-8c68-470d0844f39e)
  )
  (fp_text user "GPIO23" (at 24.13 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 924ef6ec-188f-4e9e-9e0f-8de263aaec6f)
  )
  (fp_text user "CLK" (at 24.13 45.72 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 9e31cc9b-f63e-440c-93ba-5be2fedd2590)
  )
  (fp_text user "GPIO12/MTDI" (at 1.27 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp ad64db54-4cdb-44c6-96bb-614e63a98e9c)
  )
  (fp_text user "D3" (at 1.27 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp b209d1bb-2728-4e43-b72f-94a8bf24be5e)
  )
  (fp_text user "GPIO21" (at 24.13 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp bdea339e-89d9-41cb-be78-dc080e3a5ecf)
  )
  (fp_text user "D0" (at 24.13 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp bf698fae-b050-4cab-acff-7e3db8057e31)
  )
  (fp_text user "GPIO3/U0RXD" (at 24.13 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp c313ed02-d2b0-4fe6-8c42-128c219a416e)
  )
  (fp_text user "GPIO26" (at 1.27 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp d393c47c-ae60-4f8d-bca0-fe00624e3fae)
  )
  (fp_text user "CMD" (at 1.27 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp d61a1d0b-06f4-47f2-837e-bcd69a1185d7)
  )
  (fp_text user "GPIO18" (at 24.13 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp d863c433-457a-439d-896d-49397269d2e0)
  )
  (fp_text user "GPIO14/MTMS" (at 1.27 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp f5066fdd-6a9b-47a3-abb5-bf57f9bcb805)
  )
  (fp_text user "GPIO0" (at 24.13 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp fe963dfd-d475-4a97-ba65-e59bdedaec1c)
  )
  (fp_text user "REF**" (at -0.00368 -0.00272) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dfb928c1-7d0a-4e6c-97ad-35c4a8b6679d)
  )
  (fp_line (start -1.5 46.82) (end 26.899999 46.82) (layer "F.SilkS") (width 0.12) (tstamp 13129204-7925-46ff-911b-4c3867ddb5ec))
  (fp_line (start 26.9 -1.1) (end -1.499999 -1.1) (layer "F.SilkS") (width 0.12) (tstamp 3bd4592a-100d-4661-b1b1-cb0bd780856e))
  (fp_line (start 21.71332 -7.01312) (end 21.71332 -1.12032) (layer "F.SilkS") (width 0.12) (tstamp 705cc431-56a5-482b-9826-fad3062b687f))
  (fp_line (start 3.73012 -7.01312) (end 21.71332 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp aecc5bb2-7a4e-4ea7-b827-220f978b8066))
  (fp_line (start 26.899999 46.82) (end 26.9 -1.1) (layer "F.SilkS") (width 0.12) (tstamp e10b177b-da8c-41b7-8c4f-669ea1965e3a))
  (fp_line (start -1.499999 -1.1) (end -1.5 46.82) (layer "F.SilkS") (width 0.12) (tstamp f8a56cdf-cb60-4c91-a846-ad651fa66c82))
  (fp_line (start 3.73012 -1.12032) (end 3.73012 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp ff99b65f-4fef-4d99-ae77-c4350f99a691))
  (fp_line (start -1.25 -0.85) (end 26.65 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 0521a6b8-db46-4768-9326-3e55eae52f6a))
  (fp_line (start 26.65 46.57) (end -1.25 46.57) (layer "F.CrtYd") (width 0.05) (tstamp 41f6b84f-73af-40fe-a268-110656788e7c))
  (fp_line (start -1.25 46.57) (end -1.25 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 6184f729-86eb-4b6e-9d93-18007261491e))
  (fp_line (start 26.65 -0.85) (end 26.65 46.57) (layer "F.CrtYd") (width 0.05) (tstamp 98a030ed-5018-4d4a-bec0-2613fff1433a))
  (fp_line (start -1.25 46.55) (end -1.25 -0.87) (layer "F.Fab") (width 0.1) (tstamp 473b313e-6edc-4a36-a6f8-6220900def5b))
  (fp_line (start -0.25 -0.87) (end -1.25 0.13) (layer "F.Fab") (width 0.1) (tstamp 68b6c1e5-ac93-492a-a459-bafa68a84626))
  (fp_line (start 26.65 -0.87) (end 26.65 46.55) (layer "F.Fab") (width 0.1) (tstamp 8f80e7b5-d123-4f60-8641-aa3d76af40af))
  (fp_line (start -1.25 -0.87) (end 26.65 -0.87) (layer "F.Fab") (width 0.1) (tstamp c3c03184-6ec7-46a7-9747-157ffc1a3cf2))
  (fp_line (start 26.65 46.55) (end -1.25 46.55) (layer "F.Fab") (width 0.1) (tstamp d956574e-da40-40d6-948e-ad738c3f64d0))
  (pad "1" thru_hole rect (at 0 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 92143e32-abf6-4c6d-b1ac-18a7c5240f4c))
  (pad "2" thru_hole oval (at 0 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 76e8aaf6-0107-4642-9254-afb77be4f2b2))
  (pad "3" thru_hole oval (at 0 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 906ebe3d-3f06-4824-928a-3d092ad00212))
  (pad "4" thru_hole oval (at 0 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 03548bb0-0339-4ece-a1bd-2bd3d5644be7))
  (pad "5" thru_hole oval (at 0 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e35059c8-f85e-4dbc-a85f-10d711ca53e8))
  (pad "6" thru_hole oval (at 0 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 8e6307bb-2183-4c5b-ad34-a9553438a643))
  (pad "7" thru_hole oval (at 0 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 19a531c5-62a8-45ef-8a9e-271de37dbae9))
  (pad "8" thru_hole oval (at 0 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0b937cba-d9c3-4cc0-b403-a5ac8e116d30))
  (pad "9" thru_hole oval (at 0 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 8abed457-f77e-4d2c-976e-c4c97b9760f4))
  (pad "10" thru_hole oval (at 0 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1561b085-343b-400e-91d5-31938772a140))
  (pad "11" thru_hole oval (at 0 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d9ca4a1c-a434-486a-878b-ad1a3024932a))
  (pad "12" thru_hole oval (at 0 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ee784adb-0793-439b-9cda-fbbc30073eec))
  (pad "13" thru_hole oval (at 0 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ac5ac71a-7598-43f9-a268-bd5a4f1cab97))
  (pad "14" thru_hole oval (at 0 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c9513586-73ca-4c63-8a54-3c5a6b7f8552))
  (pad "15" thru_hole oval (at 0 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ca421a89-58e7-4edc-b610-7ac1ade83fbd))
  (pad "16" thru_hole oval (at 0 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d74bc1f2-6bb1-41ab-bd77-985e9d214302))
  (pad "17" thru_hole oval (at 0 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e4f5bd7e-23ab-43b9-97ca-8fef0c15930e))
  (pad "18" thru_hole oval (at 0 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 97e07789-a6d9-4f59-ae35-417dfec7eb66))
  (pad "19" thru_hole oval (at 0 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 06977a20-8625-4fba-93b3-3223f0eff28f))
  (pad "20" thru_hole oval (at 25.39632 45.71728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp f54ae2f8-b02e-4279-a6d6-7b8c5611a4e8))
  (pad "21" thru_hole oval (at 25.39632 43.17728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 41b38318-3d8e-48d3-8d19-ba6b2fd87ca2))
  (pad "22" thru_hole oval (at 25.4 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ad09a2b1-4124-46ec-9d8d-95b5493e29c3))
  (pad "23" thru_hole oval (at 25.4 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1f04c6ef-7bf4-4e24-8bca-eeca81597ffe))
  (pad "24" thru_hole oval (at 25.4 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp fc78feeb-cdf8-4cd9-a816-e2b744df0d71))
  (pad "25" thru_hole oval (at 25.4 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b6714243-d48f-4d1f-a809-5c3d8d0c2036))
  (pad "26" thru_hole oval (at 25.4 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 29cd7555-20a1-4a22-98d8-367854629c58))
  (pad "27" thru_hole oval (at 25.4 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 8eb335cd-ade1-477d-97e1-647765f6c5b6))
  (pad "28" thru_hole oval (at 25.4 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 3dfefcbf-690d-4e68-ae53-d74054cbd2c5))
  (pad "29" thru_hole oval (at 25.4 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 71fbee5b-9390-4e56-a8d6-a5fdca8f7d90))
  (pad "30" thru_hole oval (at 25.4 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6f3e8c9e-b3d4-4ab4-b270-d668bc0a4a21))
  (pad "31" thru_hole oval (at 25.4 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 733ecf24-a477-4b8a-b1c0-9e4e43ed8db2))
  (pad "32" thru_hole oval (at 25.4 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 2165c327-623e-477b-941b-4af4ca4b77db))
  (pad "33" thru_hole oval (at 25.4 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1e5b7d72-3862-4892-a0ab-8728533ff05b))
  (pad "34" thru_hole oval (at 25.4 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 3e033a91-7b05-44c6-8b09-64a95383c0da))
  (pad "35" thru_hole oval (at 25.4 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 417e53bb-865f-40d2-8866-6f28378323ad))
  (pad "36" thru_hole oval (at 25.4 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 56a41fa8-2437-4579-85a7-e4eaf5ff0225))
  (pad "37" thru_hole oval (at 25.4 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 00ad8bbd-8725-426c-a0bf-df106ae9076e))
  (pad "38" thru_hole oval (at 25.4 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp dbc61079-b377-43ad-821d-df20bf7b5fc7))
)
