(footprint "ESP32-S2-DevKitM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 635FDC6F)
  (descr "ESP32-S2 general-purpose development board")
  (tags "ESP32-S2")
  (attr through_hole)
  (fp_text reference "REF**" (at 12.7 -2.1) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9a0b74a5-4879-4b51-8e8e-6d85a0107422)
  )
  (fp_text value "ESP32-S2-DevKitM" (at 11.42632 34.13 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eae14f5f-515c-4a6f-ad0e-e8ef233d14bf)
  )
  (fp_text user "GPIO17" (at 1.26632 45.71728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 076046ab-4b56-4060-b8d9-0d80806d0277)
  )
  (fp_text user "GPIO45" (at 21.58632 7.61728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 1171ce37-6ad7-4662-bb68-5592c945ebf3)
  )
  (fp_text user "GPIO39/MTCK" (at 21.58632 22.85728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 16121028-bdf5-49c0-aae7-e28fe5bfa771)
  )
  (fp_text user "GND" (at 21.59 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 180245d9-4a3f-4d1b-adcc-b4eafac722e0)
  )
  (fp_text user "3V3" (at 1.27 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 196a8dd5-5fd6-4c7f-ae4a-0104bd82e61b)
  )
  (fp_text user "GPIO42/MTMS" (at 21.58632 15.23728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 1fbb0219-551e-409b-a61b-76e8cebdfb9d)
  )
  (fp_text user "GPIO26" (at 21.58632 40.63728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 2454fd1b-3484-4838-8b7e-d26357238fe1)
  )
  (fp_text user "GPIO41/MTDI" (at 21.58632 17.77728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 3326423d-8df7-4a7e-a354-349430b8fbd7)
  )
  (fp_text user "GPIO13" (at 1.26632 35.55728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 3c5e5ea9-793d-46e3-86bc-5884c4490dc7)
  )
  (fp_text user "GPIO40/MTDO" (at 21.58632 20.31728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 43707e99-bdd7-4b02-9974-540ed6c2b0aa)
  )
  (fp_text user "GPIO7" (at 1.26632 20.31728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 45884597-7014-4461-83ee-9975c42b9a53)
  )
  (fp_text user "GPIO44/U0RXD" (at 21.58632 10.15728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 4db55cb8-197b-4402-871f-ce582b65664b)
  )
  (fp_text user "GPIO20/D+" (at 21.58632 45.71728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 4ec618ae-096f-4256-9328-005ee04f13d6)
  )
  (fp_text user "GPIO43/U0TXD" (at 21.58632 12.69728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 54212c01-b363-47b8-a145-45c40df316f4)
  )
  (fp_text user "GPIO5" (at 1.26632 15.23728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 6bd115d6-07e0-45db-8f2e-3cbb0429104f)
  )
  (fp_text user "GPIO10" (at 1.26632 27.93728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 79770cd5-32d7-429a-8248-0d9e6212231a)
  )
  (fp_text user "5V" (at 1.26632 48.25728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 7bfba61b-6752-4a45-9ee6-5984dcb15041)
  )
  (fp_text user "GPIO4" (at 1.26632 12.69728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 88610282-a92d-4c3d-917a-ea95d59e0759)
  )
  (fp_text user "GPIO34" (at 21.58632 35.55728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 9031bb33-c6aa-4758-bf5c-3274ed3ebab7)
  )
  (fp_text user "GPIO21" (at 21.58632 43.17728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 92035a88-6c95-4a61-bd8a-cb8dd9e5018a)
  )
  (fp_text user "GPIO8" (at 1.26632 22.85728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 97fe2a5c-4eee-4c7a-9c43-47749b396494)
  )
  (fp_text user "GPIO46" (at 21.58632 5.07728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 98914cc3-56fe-40bb-820a-3d157225c145)
  )
  (fp_text user "GPIO3" (at 1.27 10.15728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 99332785-d9f1-4363-9377-26ddc18e6d2c)
  )
  (fp_text user "GPIO38" (at 21.58632 25.39728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 99dfa524-0366-4808-b4e8-328fc38e8656)
  )
  (fp_text user "GPIO37" (at 21.58632 27.93728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 9aedbb9e-8340-4899-b813-05b23382a36b)
  )
  (fp_text user "GPIO14" (at 1.26632 38.09728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 9dcdc92b-2219-4a4a-8954-45f02cc3ab25)
  )
  (fp_text user "GPIO1" (at 1.26632 5.07728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp a32fe8ab-5810-40f6-8eab-48332c0ee5a0)
  )
  (fp_text user "GND" (at 1.26632 50.79728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp ae77c3c8-1144-468e-ad5b-a0b4090735bd)
  )
  (fp_text user "GPIO2" (at 1.26632 7.61728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b0271cdd-de22-4bf4-8f55-fc137cfbd4ec)
  )
  (fp_text user "GPIO0" (at 1.26632 2.53728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b3eebb03-af8c-48e8-a7d9-5ec3741206fa)
  )
  (fp_text user "RESET" (at 21.58632 2.53728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp c3c499b1-9227-4e4b-9982-f9f1aa6203b9)
  )
  (fp_text user "GPIO36" (at 21.58632 30.47728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp c514e30c-e48e-4ca5-ab44-8b3afedef1f2)
  )
  (fp_text user "GPIO33" (at 21.58632 38.09728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp c8b6b273-3d20-4a46-8069-f6d608563604)
  )
  (fp_text user "GPIO6" (at 1.26632 17.77728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp ce72ea62-9343-4a4f-81bf-8ac601f5d005)
  )
  (fp_text user "GPIO11" (at 1.26632 30.47728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp d0a0deb1-4f0f-4ede-b730-2c6d67cb9618)
  )
  (fp_text user "GPIO9" (at 1.26632 25.39728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp d4c9471f-7503-4339-928c-d1abae1eede6)
  )
  (fp_text user "GPIO15" (at 1.26632 40.63728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e17e6c0e-7e5b-43f0-ad48-0a2760b45b04)
  )
  (fp_text user "GPIO18" (at 21.58632 50.79728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp e4e20505-1208-4100-a4aa-676f50844c06)
  )
  (fp_text user "GPIO12" (at 1.26632 33.01728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e97b5984-9f0f-43a4-9b8a-838eef4cceb2)
  )
  (fp_text user "GPIO19/D-" (at 21.58632 48.25728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp f8f3a9fc-1e34-4573-a767-508104e8d242)
  )
  (fp_text user "GPIO35" (at 21.58632 33.01728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp fb30f9bb-6a0b-4d8a-82b0-266eab794bc6)
  )
  (fp_text user "GPIO16" (at 1.26632 43.17728 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp fea7c5d1-76d6-41a0-b5e3-29889dbb8ce0)
  )
  (fp_text user "REF**" (at -0.00368 -0.00272) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f1a9fb80-4cc4-410f-9616-e19c969dcab5)
  )
  (fp_line (start 24.35632 52.06728) (end 24.36 -1.1) (layer "F.SilkS") (width 0.12) (tstamp 3f43d730-2a73-49fe-9672-32428e7f5b49))
  (fp_line (start 20.44332 -7.01312) (end 20.44332 -1.12032) (layer "F.SilkS") (width 0.12) (tstamp 479331ff-c540-41f4-84e6-b48d65171e59))
  (fp_line (start -1.503679 52.06728) (end 24.35632 52.06728) (layer "F.SilkS") (width 0.12) (tstamp 9186dae5-6dc3-4744-9f90-e697559c6ac8))
  (fp_line (start -1.499999 -1.1) (end -1.503679 52.06728) (layer "F.SilkS") (width 0.12) (tstamp 98b00c9d-9188-4bce-aa70-92d12dd9cf82))
  (fp_line (start 24.36 -1.1) (end -1.499999 -1.1) (layer "F.SilkS") (width 0.12) (tstamp a24ce0e2-fdd3-4e6a-b754-5dee9713dd27))
  (fp_line (start 2.46012 -1.12032) (end 2.46012 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp b09666f9-12f1-4ee9-8877-2292c94258ca))
  (fp_line (start 2.46012 -7.01312) (end 20.44332 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp cc15f583-a41b-43af-ba94-a75455506a96))
  (fp_line (start -1.25368 52.06728) (end -1.25 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 1199146e-a60b-416a-b503-e77d6d2892f9))
  (fp_line (start 24.11 -0.85) (end 24.10632 52.06728) (layer "F.CrtYd") (width 0.05) (tstamp 997c2f12-73ba-4c01-9ee0-42e37cbab790))
  (fp_line (start -1.25 -0.85) (end 24.11 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp afd38b10-2eca-4abe-aed1-a96fb07ffdbe))
  (fp_line (start 24.10632 52.06728) (end -1.25368 52.06728) (layer "F.CrtYd") (width 0.05) (tstamp c8fd9dd3-06ad-4146-9239-0065013959ef))
  (pad "1" thru_hole rect (at 0 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6e435cd4-da2b-4602-a0aa-5dd988834dff))
  (pad "2" thru_hole oval (at 0 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6f675e5f-8fe6-4148-baf1-da97afc770f8))
  (pad "3" thru_hole oval (at 0 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d69a5fdf-de15-4ec9-94f6-f9ee2f4b69fa))
  (pad "4" thru_hole oval (at 0 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 917920ab-0c6e-4927-974d-ef342cdd4f63))
  (pad "5" thru_hole oval (at 0 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 8fc062a7-114d-48eb-a8f8-71128838f380))
  (pad "6" thru_hole oval (at 0 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 4f411f68-04bd-4175-a406-bcaa4cf6601e))
  (pad "7" thru_hole oval (at 0 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1fa508ef-df83-4c99-846b-9acf535b3ad9))
  (pad "8" thru_hole oval (at 0 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 155b0b7c-70b4-4a26-a550-bac13cab0aa4))
  (pad "9" thru_hole oval (at 0 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 399fc36a-ed5d-44b5-82f7-c6f83d9acc14))
  (pad "10" thru_hole oval (at 0 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp fbe8ebfc-2a8e-4eb8-85c5-38ddeaa5dd00))
  (pad "11" thru_hole oval (at 0 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 00e38d63-5436-49db-81f5-697421f168fc))
  (pad "12" thru_hole oval (at 0 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 70e4263f-d95a-4431-b3f3-cfc800c82056))
  (pad "13" thru_hole oval (at 0 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 38a501e2-0ee8-439d-bd02-e9e90e7503e9))
  (pad "14" thru_hole oval (at 0 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c0c2eb8e-f6d1-4506-8e6b-4f995ad74c1f))
  (pad "15" thru_hole oval (at 0 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp f9c81c26-f253-4227-a69f-53e64841cfbe))
  (pad "16" thru_hole oval (at 0 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 61fe4c73-be59-4519-98f1-a634322a841d))
  (pad "17" thru_hole oval (at 0 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e5864fe6-2a71-47f0-90ce-38c3f8901580))
  (pad "18" thru_hole oval (at 0 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 699feae1-8cdd-4d2b-947f-f24849c73cdb))
  (pad "19" thru_hole oval (at 0 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d88958ac-68cd-4955-a63f-0eaa329dec86))
  (pad "20" thru_hole oval (at -0.00368 48.25728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b6cd701f-4223-4e72-a305-466869ccb250))
  (pad "21" thru_hole oval (at -0.00368 50.79728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp af347946-e3da-4427-87ab-77b747929f50))
  (pad "22" thru_hole oval (at 22.85632 50.79728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e7e08b48-3d04-49da-8349-6de530a20c67))
  (pad "23" thru_hole oval (at 22.86 48.25728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 9bac9ad3-a7b9-47f0-87c7-d8630653df68))
  (pad "24" thru_hole oval (at 22.86 45.71728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 2891767f-251c-48c4-91c0-deb1b368f45c))
  (pad "25" thru_hole oval (at 22.86 43.17728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp fd3499d5-6fd2-49a4-bdb0-109cee899fde))
  (pad "26" thru_hole oval (at 22.86 40.63728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 71f92193-19b0-44ed-bc7f-77535083d769))
  (pad "27" thru_hole oval (at 22.86 38.09728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 143ed874-a01f-4ced-ba4e-bbb66ddd1f70))
  (pad "28" thru_hole oval (at 22.86 35.55728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 795e68e2-c9ba-45cf-9bff-89b8fae05b5a))
  (pad "29" thru_hole oval (at 22.86 33.01728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 8fcec304-c6b1-4655-8326-beacd0476953))
  (pad "30" thru_hole oval (at 22.86 30.47728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 411d4270-c66c-4318-b7fb-1470d34862b8))
  (pad "31" thru_hole oval (at 22.86 27.93728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0520f61d-4522-4301-a3fa-8ed0bf060f69))
  (pad "32" thru_hole oval (at 22.86 25.39728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c8b92953-cd23-44e6-85ce-083fb8c3f20f))
  (pad "33" thru_hole oval (at 22.86 22.85728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp bc0dbc57-3ae8-4ce5-a05c-2d6003bba475))
  (pad "34" thru_hole oval (at 22.86 20.31728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 00f3ea8b-8a54-4e56-84ff-d98f6c00496c))
  (pad "35" thru_hole oval (at 22.86 17.77728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 009b5465-0a65-4237-93e7-eb65321eeb18))
  (pad "36" thru_hole oval (at 22.86 15.23728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 221bef83-3ea7-4d3f-adeb-53a8a07c6273))
  (pad "37" thru_hole oval (at 22.86 12.69728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b52d6ff3-fef1-496e-8dd5-ebb89b6bce6a))
  (pad "38" thru_hole oval (at 22.86 10.15728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 4ba06b66-7669-4c70-b585-f5d4c9c33527))
  (pad "39" thru_hole oval (at 22.86 7.61728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 60ff6322-62e2-4602-9bc0-7a0f0a5ecfbf))
  (pad "40" thru_hole oval (at 22.86 5.07728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e7369115-d491-4ef3-be3d-f5298992c3e8))
  (pad "41" thru_hole oval (at 22.86 2.53728 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp aa130053-a451-4f12-97f7-3d4d891a5f83))
  (pad "42" thru_hole oval (at 22.86 -0.00272 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 9186fd02-f30d-4e17-aa38-378ab73e3908))
)
