(footprint "ESP32-S2-Saola-1" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 635FDA23)
  (descr "Espressif ESP32-S2-Saola-1 Development Kit: https://docs.espressif.com/projects/esp-idf/en/latest/esp32s2/hw-reference/esp32s2/user-guide-saola-1-v1.2.html")
  (tags "esp32-s2 devkit")
  (attr through_hole)
  (fp_text reference "REF**" (at 12.7 -2.1) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1e3f934c-e526-46f7-91dc-0281bb60506e)
  )
  (fp_text value "ESP32-S2-Saola-1" (at 12.7 24.13 90) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0e7b9fdc-b555-49c7-8ba2-702da493bde4)
  )
  (fp_text user "GPIO18" (at 24.13 50.8 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 00bd6ee7-9e10-4fd6-b1e6-67f0e13812f6)
  )
  (fp_text user "GPIO34" (at 24.13 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 02c6068b-19c4-4372-b901-805eb488afa5)
  )
  (fp_text user "GPIO20/USB_D+" (at 24.13 45.72 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 05313705-1375-46fe-b46f-56a06006da3d)
  )
  (fp_text user "GPIO2" (at 1.27 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 065bdab4-0ab0-4a01-acd8-f2897436e6e3)
  )
  (fp_text user "GPIO9" (at 1.27 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 08fd7a13-7ca4-4701-9d84-096bc8215616)
  )
  (fp_text user "1" (at -2.00368 -0.00272) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0f159094-9f3b-434c-9eb3-748cce593b06)
  )
  (fp_text user "GPIO6" (at 1.27 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 2c89ffab-8108-4540-ba05-cf929c82cf9e)
  )
  (fp_text user "22" (at 27.94632 50.79728) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 342253f4-3f38-46f7-a243-5b8a83885538)
  )
  (fp_text user "GPIO33" (at 24.13 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 3a047cbc-1fd8-4fcf-a88f-fa60c232af94)
  )
  (fp_text user "GPIO40/MTDO" (at 24.13 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 47ccf195-8a1d-462e-903e-4e043330e611)
  )
  (fp_text user "GPIO37" (at 24.13 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 4daa00d5-dc8b-462d-ad58-5ea399b2a01a)
  )
  (fp_text user "GPIO26" (at 24.13 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 5e79ab5d-8bfd-4ce9-bd2e-28cccf1128ff)
  )
  (fp_text user "GPIO3" (at 1.27 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 60bbf9c1-ff20-401e-a3d9-962a4f028bae)
  )
  (fp_text user "GPIO39/MTCK" (at 24.13 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 6e85bc3f-8df5-43f9-8203-44b0594ecfb6)
  )
  (fp_text user "GPIO8" (at 1.27 22.86 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 7025b3c1-4bab-4ea9-9583-8aa24d915007)
  )
  (fp_text user "GPIO10" (at 1.27 27.94 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 71511879-11a4-470e-a548-e5ebcd150156)
  )
  (fp_text user "GPIO11" (at 1.27 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 75f2f233-bd55-42d8-ac99-0909bc4a83a9)
  )
  (fp_text user "GPIO41/MTDI" (at 24.13 17.78 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 768ff47a-5e33-40ca-abc4-44e355cd1b5a)
  )
  (fp_text user "EN/RESET" (at 24.13 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 7fc28a8c-418a-4a65-9519-b798088af73b)
  )
  (fp_text user "IO45" (at 24.13 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 88008ede-aa42-42aa-9c15-899f6feeb22b)
  )
  (fp_text user "GPIO1" (at 1.27 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 8afd9731-865f-4fdb-97b7-96f68a16227b)
  )
  (fp_text user "GPIO4" (at 1.27 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 8c9a20b4-a23b-4f82-b119-b96df431fef4)
  )
  (fp_text user "GPIO44/U0RXD" (at 24.13 10.16 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 8ea929a8-c616-4ec2-88c7-f9a6ccb2ab09)
  )
  (fp_text user "GND" (at 24.13 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 8ed3d9eb-7c42-4f22-a581-a1d81dac918c)
  )
  (fp_text user "GPIO5" (at 1.27 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp 91529ed0-bf93-44a8-b220-9db1373d7fbc)
  )
  (fp_text user "GPIO38" (at 24.13 25.4 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp 934dd71f-c374-43a8-96d2-532b75148d4c)
  )
  (fp_text user "5V" (at 1.27 48.26 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 9f890831-687f-4e51-ae23-64de99460f8e)
  )
  (fp_text user "GND" (at 1.27 50.8 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b085d6cf-18ef-49ad-a797-29cc6f5bdbec)
  )
  (fp_text user "GPIO19/USB_D-" (at 24.13 48.26 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp b2199a7f-ed5b-488b-88b7-29acd2319bb6)
  )
  (fp_text user "GPIO13" (at 1.27 35.56 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp b5254efc-e40f-4fef-bd79-a3074bc99a15)
  )
  (fp_text user "3V3" (at 1.27 0 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b9f289f5-7e62-463b-844a-4eced3564c42)
  )
  (fp_text user "GPIO14" (at 1.27 38.1 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp bdb4c561-7f21-4a5d-94c8-b78c4028401d)
  )
  (fp_text user "GPIO36" (at 24.13 30.48 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp c4c8c7d1-d7da-4204-8d71-1d756ea2ec9e)
  )
  (fp_text user "GPIO35" (at 24.13 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp cc3ef39f-6be8-4415-8184-09e398c87c89)
  )
  (fp_text user "GPIO15" (at 1.27 40.64 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp cd852aa4-baff-4562-8d96-fd48557cd8e5)
  )
  (fp_text user "GPIO7" (at 1.27 20.32 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp d4ecf6ad-81d5-410d-bf6f-63cb5b36b99d)
  )
  (fp_text user "GPIO21" (at 24.13 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp d8972b07-a589-4865-97ac-13ce652b8afd)
  )
  (fp_text user "GPIO43/U0TXD" (at 24.13 12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp df0d084b-0372-4cbf-950c-960a6cdaaa71)
  )
  (fp_text user "GPIO16" (at 1.27 43.18 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp e52b1490-6e36-457c-9fee-1be3bceb9cdc)
  )
  (fp_text user "GPIO17" (at 1.27 45.72 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp ede460ad-8fee-4c65-83c4-9f93dbcf6aa6)
  )
  (fp_text user "GPIO0/BOOT" (at 1.27 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp f14f3731-133b-4f3a-a52a-fd3f73c4e401)
  )
  (fp_text user "GPIO42/MTMS" (at 24.13 15.24 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp f6dcc3cc-3358-449d-bfeb-aa73d93b7dbe)
  )
  (fp_text user "GPIO12" (at 1.27 33.02 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify left))
    (tstamp fdd408f2-13fb-4011-adde-2b11edec2cf0)
  )
  (fp_text user "IO46" (at 24.13 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify right))
    (tstamp fff596bc-5b80-4506-a1f8-342c3370491c)
  )
  (fp_text user "REF**" (at -0.00368 -0.00272) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fb7c2316-3825-4403-8132-8f1450ea7c1c)
  )
  (fp_line (start 26.9 -1.1) (end -1.499999 -1.1) (layer "F.SilkS") (width 0.12) (tstamp 2957caf4-cb4a-4e4f-b36f-763b4c91b76f))
  (fp_line (start -1.5 51.9) (end 26.899999 51.9) (layer "F.SilkS") (width 0.12) (tstamp 38fe9548-2892-4086-9132-56eca0613172))
  (fp_line (start -1.499999 -1.1) (end -1.5 51.9) (layer "F.SilkS") (width 0.12) (tstamp 49ba0a93-4a2a-4833-ab81-6f80362ccbc7))
  (fp_line (start 21.68792 -7.01312) (end 21.68792 -1.12032) (layer "F.SilkS") (width 0.12) (tstamp 968b334c-dab0-4288-8e8f-ed7332a78dc1))
  (fp_line (start 3.70472 -7.01312) (end 21.68792 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp 9fd03fd1-19cb-4fba-ada9-de526306bceb))
  (fp_line (start 3.70472 -1.12032) (end 3.70472 -7.01312) (layer "F.SilkS") (width 0.12) (tstamp e4ef9eac-1551-4212-9e34-a254f208efca))
  (fp_line (start 26.899999 51.9) (end 26.9 -1.1) (layer "F.SilkS") (width 0.12) (tstamp e99e43a3-ed91-4503-9993-e825d17ca21b))
  (fp_line (start 26.65 -0.85) (end 26.65 51.65) (layer "F.CrtYd") (width 0.05) (tstamp 01792d0e-7b8c-4865-abbb-3ab8eda38fdc))
  (fp_line (start -1.25 -0.85) (end 26.65 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 14f91e95-12c9-4040-86a4-3ad5d2ce2228))
  (fp_line (start -1.25 51.65) (end -1.25 -0.85) (layer "F.CrtYd") (width 0.05) (tstamp 5e61582a-5ee2-46fc-add7-9f41f888484a))
  (fp_line (start 26.65 51.65) (end -1.25 51.65) (layer "F.CrtYd") (width 0.05) (tstamp 74c8de49-d250-4172-8582-023c2562cba1))
  (pad "1" thru_hole rect (at 0 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 165058a7-dbd0-4c41-9cc5-d3eeb49b401e))
  (pad "2" thru_hole oval (at 0 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0f45ae42-da35-492f-84e7-9fcec4e38431))
  (pad "3" thru_hole oval (at 0 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e261a752-1c99-44c3-aa2d-69ce7a1b515b))
  (pad "4" thru_hole oval (at 0 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp bccfdf62-5f89-473c-8c8c-192fd1874ce2))
  (pad "5" thru_hole oval (at 0 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d7c26768-5e67-445c-814e-0530dfbb49a5))
  (pad "6" thru_hole oval (at 0 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 3c792e11-cf7c-487b-ae0e-b26a473e6084))
  (pad "7" thru_hole oval (at 0 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0a5759d6-fa3e-4a54-99da-e4b4faa94aa3))
  (pad "8" thru_hole oval (at 0 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp f0bdbcbc-e896-4c85-94bb-04513ade3a43))
  (pad "9" thru_hole oval (at 0 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 706bb5d5-95e2-427d-9129-f6674bbf3ab0))
  (pad "10" thru_hole oval (at 0 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 632e6545-ddd9-4118-9c72-fb107f42762b))
  (pad "11" thru_hole oval (at 0 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ba2a31bc-008e-413a-96be-2724be9e8a90))
  (pad "12" thru_hole oval (at 0 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp a5f020ed-839e-4153-b06e-c0582a228928))
  (pad "13" thru_hole oval (at 0 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 2fd4c60d-a128-40c0-abf7-24d7934aaaaa))
  (pad "14" thru_hole oval (at 0 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 4e12c7b0-1c7b-4d9b-8daa-d4690c1d0fbb))
  (pad "15" thru_hole oval (at 0 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 4364c09c-337f-40a5-8827-4245f871fcdb))
  (pad "16" thru_hole oval (at 0 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 97becc95-fece-4dfc-8063-da49934c95e8))
  (pad "17" thru_hole oval (at 0 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1559d0e8-4b43-45c7-b09f-c64bae059386))
  (pad "18" thru_hole oval (at 0 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp dcd9789c-9f36-4ff4-b1a6-d44ed6bf51db))
  (pad "19" thru_hole oval (at 0 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d9c83668-a39c-4ee6-8585-715ea5cbbe15))
  (pad "20" thru_hole oval (at 0 48.26 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6345ad24-18f6-4e6a-9c5c-132a0fb7e8c7))
  (pad "21" thru_hole oval (at 0 50.8 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp f14818b1-4187-4793-a83a-510d3b6135c8))
  (pad "22" thru_hole oval (at 25.4 50.8 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp c9e2a3b3-0d93-4c64-87b6-b215f63ea4a7))
  (pad "23" thru_hole oval (at 25.4 48.26 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 63990f30-5409-4701-89d0-1e40fb4761b9))
  (pad "24" thru_hole oval (at 25.4 45.72 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 662a7a56-4252-4c8f-9afc-7ed719a5b122))
  (pad "25" thru_hole oval (at 25.4 43.18 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 7954fade-11e5-41e7-8139-595f1d7df616))
  (pad "26" thru_hole oval (at 25.4 40.64 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp cd0c74bc-2f72-4628-a79c-0abe1afb54f4))
  (pad "27" thru_hole oval (at 25.4 38.1 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 40ef6eac-9e85-425d-a969-638ddd63abd6))
  (pad "28" thru_hole oval (at 25.4 35.56 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e3e1bf41-4b63-4094-b14c-8439536f0807))
  (pad "29" thru_hole oval (at 25.4 33.02 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp d9ae6c20-9c65-4489-85ac-b6b82b547b3c))
  (pad "30" thru_hole oval (at 25.4 30.48 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp bed2e0a9-3d7d-4550-a48a-f7dbbc9967bf))
  (pad "31" thru_hole oval (at 25.4 27.94 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 47b062c8-bceb-4c38-b579-1f6db78bc9c0))
  (pad "32" thru_hole oval (at 25.4 25.4 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp dc9130e2-0a96-49e6-93a3-5f661cc42da4))
  (pad "33" thru_hole oval (at 25.4 22.86 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b5a2e2a0-c130-44f3-b9a3-4ff12a04e4c4))
  (pad "34" thru_hole oval (at 25.4 20.32 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp ca421d61-605e-4e2d-9a4d-058fc5bfbcca))
  (pad "35" thru_hole oval (at 25.4 17.78 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp a4a212d4-334b-4b7c-b4fe-5bc1e155f519))
  (pad "36" thru_hole oval (at 25.4 15.24 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 567aeecb-31a7-4d28-9b2d-903a2a3708e7))
  (pad "37" thru_hole oval (at 25.4 12.7 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1b6ad88b-eba5-49c6-974b-e9b90dc30a12))
  (pad "38" thru_hole oval (at 25.4 10.16 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 78fdc2ca-36fc-470c-a12f-f06bae612028))
  (pad "39" thru_hole oval (at 25.4 7.62 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 18c1ce71-6f22-4edf-8cd4-9f2528e03d30))
  (pad "40" thru_hole oval (at 25.4 5.08 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp 196729df-86bc-4d33-b4ae-6ebc742fde28))
  (pad "41" thru_hole oval (at 25.4 2.54 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp e17d8122-dea1-4f55-be00-69355d2d6b4b))
  (pad "42" thru_hole oval (at 25.4 0 270) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask) (tstamp b164a8b0-9ac3-4e00-9379-8761a7e3b53d))
)
